


K12 Bollard - PAS68 Static Bollards – ESF – SIM - T50ST





* PAS68: V/7500[N2]/80/90:1.0/21.2 Certified.
* Bollard tested with N2 & N3 7.5ton vehicle at 50mph / 80kmh
* Diameter: 273mm
* Height: 1000mm above FFL
* Finish: Stainless-Steel Sleeve
* Foundation: 750mm, plus 75mm blinding and allowance for 100mm topping.
* Static fixed option.
* Test Certificate Supplied